**MOORING INSPECTION REPORT**

|  |  |  |  |
| --- | --- | --- | --- |
| **Mooring ID** | RIA01 | **Mooring Control Area** | Thomson Bay |
| **Easting** | 362549.5 | **MMD Centre** | 2.5m |
| **Northing** | 6459173.6 | **MMD in MSR** | 2.3m |
| **Maximum Vessel Length** | 14m | **Tonnage** | 20t |
| **Maximum Swing Room** | 35.1m | **Buoy Swing Radius** | 3.12m |
| **Distance to Nearest Mooring** |  | **ID of Nearest Mooring** |  |
| **Diver** |  | **Inspection Date** |  |

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **Components** | **Description** | **2020 Inspection** | **2021 Inspection %** | **Size of Chain (mm)** | **Comments** |
| Surface Buoy | Green 800mmAqualib Buoy | Good |  |  |  |
| SF Mooring ID Number \* | RIA01 |  |  |  |  |  |
| Disc Colour | Purple |  |  |  |  |
| Labelling |  |  |  |  |  |
| Super Tender Certified | Up to 6.75m | Yes |  |  |  |
| Max Wind Strength | 40 Knots |  |  |  |  |
| Pick up Line | 4m x 28mm Nylon Y | New |  |  |  |
| Pimple Floats |  |  |  |  |  |
| Shackle |  |  |  |  |  |
| Buoy Shaft | 1m x 19mm /S Swivel Shaft | Good |  |  |  |
| Shackle |  |  |  |  |  |
| Swivel | 16mm S/S on shaft | Good |  |  |  |
| Shackle |  |  |  |  |  |
| Pendant Chain | 4m x 16mm Chain | Good |  |  |  |
| Sub Surface Float | 300mm | Good |  |  |  |
| Shackle | 4.75T Green Pin Safety Bow | Good |  |  |  |
| Bullring | 6.5T Green Pin Safety Bow | Good |  |  |  |
| **Ground Chain 1** |  |  |  |  |  |
| Ground Chain 1 | 5m x 28mm Chain | Average |  |  |  |
| Shackle to Bullring |  |  |  |  |  |
| Shackle to Anchor |  |  |  |  |  |
| Anchor | 2m x Vertical Pin | Buried |  |  |  |
| **Ground Chain 2** |  |  |  |  |  |
| Ground Chain 2 | 5m x 28mm Chain | Average |  |  |  |
| Shackle to Bullring |  |  |  |  |  |
| Shackle to Anchor |  |  |  |  |  |
| Anchor | 2m x Vertical Pin | Buried |  |  |  |
| **Ground Chain 3** |  |  |  |  |  |
| Ground Chain 3 | 5m x 28mm Chain | Average |  |  |  |
| Shackle to Bullring |  |  |  |  |  |
| Shackle to Anchor |  |  |  |  |  |
| Anchor | 2m x Vertical Pin | Buried |  |  |  |

|  |  |
| --- | --- |
| **KEY TO CONDITION OF COMPONENTS** | |
| **1%** NEW FITTED  **2% - 29%** GOOD CONDITION | **30% - 39%** AVERAGE CONDITION  **40%** AND OVER POOR CONDITION |
| **MOORING PHOTO** | **GENERAL OBSERVATION** |
|  |  |

\*All stickers and discs to be intact and clearly legible on the surface float

**MOORING IS SAFE and FIT FOR PURPOSE** □

**ENVIRONMENTALLY FRIENDLY MOORING** □

**MOORING CONTRACTOR DECLARATION**

I, Adam Falconer-West on behalf of Franmarine Underwater Services Pty Ltd certify that the abovementioned mooring was inspected by our diving team in accordance with Australian Standard AS2299. The information contained in this Report is true and correct and the mooring is SAFE and FIT FOR PURPOSE to hold a vessel up to the maximum vessel length in up to 40 knot winds for 12 months from the date of this certification.

|  |  |
| --- | --- |
| **Signed:** | **Date:** |

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **Arrival Time** |  | **Bottom Time** |  | **Departure Time** |  |